
Log Written: Monday, October 25, 21:15:36 Центральная Азия (зима)
MP FSN: B06011600078010
MP Name: MP 555 GPS
MP Firmware: R2_3_2AP C:/PROJ/TEMP/R2_3_2AP/FW 2007/05/01 18:07:12
Modem Firmware: R2_2_2_5AC_VZW F:/AC555VZW/ROSETTA 2004/10/14 16:11:25
************************** Log Start **************************
Searching for connected MP...
TX: ati4
RX: 

630FD9DF
OK

TX: ati5
RX: 

R2_3_2AP
OK

TX: at!MPCFGDUMP?1
RX: 

I4
630FD9DF
I5
R2_3_2AP
I6
R1_0_0mp750bt
&V
ACTIVE PROFILE:

E1  L0  M0  Q0  V1  X4  &C1  &D2
S0:0  S1:0  S2:0  S3:13  S4:10  S5:8
S6:2  S7:60  S8:2  S10:15  S12:0  S13:0
+IFC:2,2
+IPR:115200

+GMM
MP555
+GMR
R2_3_2AP
!MPGVER?
R2_3_2AP C:/PROJ/TEMP/R2_3_2AP/FW 2007/05/01 18:07:12
!MPFBTIME?
!MPFBTIME: 60
!MPIDTIME?
!MPIDTIME: 2
!MPBARSVC?
!MPBARSVC: 0
!MPSETDFLT?
!MPSETDFLT: 1
!MPOPMODE?
!MPOPMODE: 0
!MPSETUP?1
1:MP 1X (High-Speed),7009231940@vzw3g.com,vzw,#777
!MPSETUP?2
2:MP Quick Net Connect,dalacom,dalacom,#762
!MPSETUP?3
3:,,,
!MPFBSETUP?
,,,
!MPPDDELAY?
0
!MPPRIVIP?
95.56.55.244,2103,2104
!MPCLIENTIP?
IP:      0.0.0.0
Pri DNS: 0.0.0.0
Sec DNS: 0.0.0.0
!MPPADSETUP?
0,0.0.0.0,0,0
!MPPADCONF?
0,0,1,1,13,1460,1,1,8
!MPPRODID?
0x00
!MPPCBREV?
0x04
!MPMTCONF?0
0,0,0.0.0.0,0,5,3,10
!MPMTCONF?1
1,0,0.0.0.0,0,5,3,10
!MPMTCONF?2
2,0,0.0.0.0,0,5,3,10
!MPMTCONF?3
3,0,0.0.0.0,0,5,3,10
!MPIGNSENSE?
1
!MPCONFSNAP?
7627,21000,0
!MPRESETCNT?
MPRESETCNT: 
MP: 12
AT-Start-trig MP: 0
CM-Recover-trig MP: 0
BS-ACreset-trig MP: 0
AirCard: 22
CM-trig AC: 0
ATdisc-trig AC: 0
AC rst fail: 0
!MPPANDP?
MPPANDP: 0

!MPUSB?
1
!MPAUTHPPP?
0
!MPGPSSTOR?
0
!MPRECON?
!MPRECON: 0
!MPWATCHER?
0,0
OK

TX: at!MPCFGDUMP?2
RX: 

!MPDIOCFG?1
1
255
INPUT
0
LOW
HIGH
255
!MPDIOCFG?2
2
255
INPUT
0
LOW
HIGH
255
!MPDIOCFG?3
3
255
INPUT
0
LOW
HIGH
255
!MPDIOCFG?4
4
255
INPUT
0
LOW
HIGH
255
!MPAINCFG?1
1
ANALOG1
NA
0
1023
!MPAINCFG?2
2
ANALOG2
NA
0
1023
!MPAINCFG?3
3
ANALOG3
NA
0
1023
!MPAINCFG?4
4
ANALOG4
NA
0
1023
!MPGPSST?
State: 2
Recv Drop: 0
Recv Len Drop: 0
Max Rx Buf Used: 9
Reset Cnt: 0
Protocol: 0
InitBaudRate: 9600
localUpdateInt: 1
rmFlag: 31
Init Str 1: 
Init Str 2: 
Init Str 3: 
Init Str 4: 
Init Str 5: 
!MPGPSNMEA?
0,1,0,1,0,0,1
!MPGPSTAIP?
1,0,0,0,0
!MPGPSESC?
0
!MPGPSTRACK?
0
!MPCWSETUP?
!MPCWSETUP: 0,30,7367,www.sierrawireless.com,0,0.0.0.0,0
!MPCWINFO?
MPCWINFO: 
CW state: Not connected
DNS/PING checks (NV):         0
Consecutive disconnects: 0
CW-trig disconnect (NV): 0
CW-trig AC resets (NV):  0
Total TX bytes by CW while in CWON: 0
Total RX bytes by CW while in CWON: 0
Total TX bytes by CW while in CWVERIFY: 0
Total RX bytes by CW while in CWVERIFY: 0
!MPCONREJ?
!MPCONREJ: 0
OK

TX: at!mpclientip?
RX: 

IP:      0.0.0.0
Pri DNS: 0.0.0.0
Sec DNS: 0.0.0.0
OK


Finished

*************************** Log End ***************************
